**Static Routing Project**

A diagram of a computer network

AI-generated content may be incorrect.

**Addressing Table**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Device** | **Interface** | **IP Address** | **Subnet Mask** | **Default Gateway** | **VLAN** |
| R1 | S0/0/0 | 172.31.1.2 | 255.255.255.0 | N/A | N/A |
| G0/0.10 | 172.31.10.1 | 255.255.255.0 | N/A | 10 |
| G0/0.20 | 172.31.20.1 | 255.255.255.0 | N/A | 20 |
| G0/0.30 | 172.31.30.1 | 255.255.255.0 | N/A | 30 |
| G0/0.88 | 172.31.88.1 | 255.255.255.0 | N/A | 88 |
| G0/0.99 | 172.31.99.1 | 255.255.255.0 | N/A | 99 |
| S1 | VLAN 88 | 172.31.88.33 | 255.255.255.0 | 172.31.88.1 | 88 |
| PC-A | NIC | 172.31.10.21 | 255.255.255.0 | 172.31.10.1 | 10 |
| PC-B | NIC | 172.31.20.22 | 255.255.255.0 | 172.31.20.1 | 20 |
| PC-C | NIC | 172.31.30.23 | 255.255.255.0 | 172.31.30.1 | 30 |
| PC-D | NIC | 172.31.88.24 | 255.255.255.0 | 172.31.88.1 | 88 |

**VLAN Table**

|  |  |  |
| --- | --- | --- |
| **VLAN** | **Name** | **Interfaces** |
| 10 | Sales | F0/11-15 |
| 20 | Production | F0/16-20 |
| 30 | Marketing | F0/5-10 |
| 88 | Management | F0/21-24 |
| 99 | Native | G1/1 |

**Scenario**

In this activity, you will demonstrate and reinforce your ability to configure routers for inter-VLAN communication and configure static routes to reach destinations outside of your network. Among the skills you will demonstrate are configuring inter-VLAN routing, static and default routes.

**Requirements**

·         Configure inter-VLAN routing on **R1** based on the **Addressing Table**.

·         Configure trunking on **S1**.

·         Configure four directly attached static route on **HQ** to each VLANs 10, 20, 30 and 88.

·         Configure directly attached static routes on **HQ** to reach **Outside Host**.

-       Configure the primary path through the Serial 0/1/0 interface.

-       Configure the backup route through the Serial 0/1/1 interface with a 10 AD.

·         Configure directly attached primary and backup summary routes on **ISP** for the entire 172.31.0.0/17 address space.

-       Configure the primary path through the Serial 0/1/1 interface.

-       Configure the backup route through the Serial 0/1/0 interface with 25 AD.

·         Configure a directly attached default route on **R1**.

·         Verify connectivity by making sure all the PCs can ping **Outside Host**.